# Rafael Carvalho Matias, Jérôme Ouellet.

## Configuration R1 :

Building configuration...

Current configuration : 940 bytes

!

version 15.4

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname R1

!

no ip cef

no ipv6 cef

!

spanning-tree mode pvst

!

interface GigabitEthernet0/0/0

no ip address

duplex auto

speed auto

shutdown

!

interface GigabitEthernet0/0/1

ip address 198.96.120.254 255.255.248.0

duplex auto

speed auto

!

interface GigabitEthernet0/0/2

no ip address

duplex auto

speed auto

shutdown

!

interface Serial0/2/0

ip address 198.96.252.1 255.255.255.252

!

interface Serial0/2/1

ip address 198.96.252.9 255.255.255.252

!

interface Vlan1

no ip address

shutdown

!

ip classless

ip route 198.96.252.0 255.255.252.0 198.96.252.2

ip route 198.96.112.0 255.255.240.0 198.96.252.5

ip route 198.96.128.0 255.255.248.0 198.96.252.10

!

ip flow-export version 9

!

line con 0

!

line aux 0

!

line vty 0 4

login

!

End

## Configuration R2 :

Building configuration...

Current configuration : 959 bytes

!

version 15.4

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname R2

!

no ip cef

no ipv6 cef

!

spanning-tree mode pvst

!

interface GigabitEthernet0/0/0

no ip address

duplex auto

speed auto

shutdown

!

interface GigabitEthernet0/0/1

ip address 198.96.112.254 255.255.240.0

duplex auto

speed auto

!

interface GigabitEthernet0/0/2

no ip address

duplex auto

speed auto

shutdown

!

interface Serial0/2/0

ip address 198.96.252.2 255.255.255.252

clock rate 2000000

!

interface Serial0/2/1

ip address 198.96.252.5 255.255.255.252

!

interface Vlan1

no ip address

shutdown

!

ip classless

ip route 198.96.252.0 255.255.252.0 198.96.252.1

ip route 198.96.120.0 255.255.248.0 198.96.252.1

ip route 198.96.128.0 255.255.248.0 198.96.252.6

!

ip flow-export version 9

!

line con 0

!

line aux 0

!

line vty 0 4

login

!

End

## Configuration R3 :

Building configuration...

Current configuration : 930 bytes

!

version 15.4

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname R3

!

no ip cef

no ipv6 cef

!

spanning-tree mode pvst

!

interface GigabitEthernet0/0/0

no ip address

duplex auto

speed auto

shutdown

!

interface GigabitEthernet0/0/1

ip address 198.96.128.254 255.255.252.0

duplex auto

speed auto

!

interface GigabitEthernet0/0/2

no ip address

duplex auto

speed auto

shutdown

!

interface Serial0/2/0

ip address 198.96.252.10 255.255.255.252

clock rate 2000000

!

interface Serial0/2/1

ip address 198.96.252.6 255.255.255.252

clock rate 2000000

!

interface Vlan1

no ip address

shutdown

!

ip classless

ip route 198.96.120.0 255.255.248.0 198.96.252.9

ip route 198.96.112.0 255.255.240.0 198.96.252.5

!

ip flow-export version 9

!

line con 0

!

line aux 0

!

line vty 0 4

login

!

end